IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2021-06-23T10:14:13"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20160225_1515(x64) - Exporter 17.0.416.0 - Alternate UI 17.12.14.0"
Application: "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)"

People and organizations
  Person "sezer.yildirim3XTPN" of Organization (no name given)
  Owner history of Person "sezer.yildirim3XTPN" of Organization (no name given) | application "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)" | change NOCHANGE | created 1623424259 (2021-06-11T15:10:59Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING | postal address: "## Street City, State Zip", "Boston", "MA"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCFLOWTERMINAL | object type "ConcealedCistern-ForWallHungWCPans-3/6lt-WithAdjustableThickMetalFeet-8cm-FloorMounting-VitrA-768-1850-01" | names: "ConcealedCistern-ForWallHungWCPans-8cm-WithAdjustableThinMetalFeet-VitrA-768-1851:ConcealedCistern-ForWallHungWCPans-3/6lt-WithAdjustableThickMetalFeet-8cm-FloorMounting-VitrA-768-1850-01:1565714" | material: materials ("Console", "Black", "White", "Orange") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Constraints, Dimensions, Identity Data, Mechanical

Property sets
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "## Street City, State Zip" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "Project Number" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other | properties | on 1 object (1 IFCFLOWTERMINAL)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family = "ConcealedCistern-ForWallHungWCPans-8cm-WithAdjustableThinMetalFeet-VitrA-768-1851: ConcealedCistern-ForWallHungWCPans-3/6lt-WithAdjustableThickMetalFeet-8cm-FloorMounting-VitrA-768-1850-01" (IFCLABEL)
    Family and Type = "ConcealedCistern-ForWallHungWCPans-8cm-WithAdjustableThinMetalFeet-VitrA-768-1851: ConcealedCistern-ForWallHungWCPans-3/6lt-WithAdjustableThickMetalFeet-8cm-FloorMounting-VitrA-768-1850-01" (IFCLABEL)
    Schedule Level = "Level: Level 1" (IFCLABEL)
    Type = "ConcealedCistern-ForWallHungWCPans-8cm-WithAdjustableThinMetalFeet-VitrA-768-1851: ConcealedCistern-ForWallHungWCPans-3/6lt-WithAdjustableThickMetalFeet-8cm-FloorMounting-VitrA-768-1850-01" (IFCLABEL)
    Type Id = "ConcealedCistern-ForWallHungWCPans-8cm-WithAdjustableThinMetalFeet-VitrA-768-1851: ConcealedCistern-ForWallHungWCPans-3/6lt-WithAdjustableThickMetalFeet-8cm-FloorMounting-VitrA-768-1850-01" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Other | properties | on 1 object (1 IFCFLOWTERMINAL)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family Name = "ConcealedCistern-ForWallHungWCPans-8cm-WithAdjustableThinMetalFeet-VitrA-768-1851" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWTERMINAL)
    Mark = "472" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCFLOWTERMINAL)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Brand = "Vitra" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "VitrA Concealed Cistern for Wall-Hung WC Pans Standart Installation Set - Adjusted to 3/6lt - 8 cm" (IFCTEXT)
    EAN code = "" (IFCTEXT)
    Features = "" (IFCTEXT)
    GTIP code = "" (IFCTEXT)
    Installation instructions = "" (IFCTEXT)
    Manufacturer = "Vitra" (IFCTEXT)
    Model = "768-1850-01" (IFCTEXT)
    OmniClass Number = "23.45.00.00" (IFCTEXT)
    OmniClass Title = "Sanitary, Laundry, and Cleaning Equipment" (IFCTEXT)
    Product Guid = "" (IFCTEXT)
    Product certification = "https://www.vitraglobal.com/brochures/" (IFCTEXT)
    Product data url = "" (IFCTEXT)
    Product url = "https://www.vitra.com.tr/" (IFCTEXT)
    Specification = "" (IFCTEXT)
    Technical description = "https://www.vitra.com.tr/" (IFCTEXT)
    Type Name = "ConcealedCistern-ForWallHungWCPans-3/6lt-WithAdjustableThickMetalFeet-8cm-FloorMounting-VitrA-768-1850-01" (IFCTEXT)
    URL = "https://www.vitra.com.tr/" (IFCTEXT)
    Youtube = "https://www.youtube.com/user/VitrAglobal" (IFCTEXT)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCFLOWTERMINAL)
    Manufacturer = "Vitra" (IFCLABEL)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWTERMINAL)
    Reference = "ConcealedCistern-ForWallHungWCPans-3/6lt-WithAdjustableThickMetalFeet-8cm-FloorMounting-VitrA-768-1850-01" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCFLOWTERMINAL)
    Elevation = 9774.69307171872 (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "<not associated>" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCFLOWTERMINAL)
    Default Elevation = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Dimensions | properties | on 1 object (1 IFCFLOWTERMINAL)
    Area = 0.783667894756755 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.0488018486774499 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWTERMINAL)
    Nominal Depth (mm) = 80. (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Height (mm) = 1100. (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Width (mm) = 500. (IFCLENGTHMEASURE) [MILLI METRE]
    Outlet Angle = 45. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Mechanical | properties | on 1 object (1 IFCFLOWTERMINAL)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Sanitary,Domestic Cold Water" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCFLOWTERMINAL)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Data | properties | on 1 object (1 IFCFLOWTERMINAL)
    Accessories (default) = "" (IFCTEXT)
    Article No. (default) = "768-1850-01" (IFCTEXT)
    Calculated flow = "" (IFCTEXT)
    Color = "" (IFCTEXT)
    Tap hole Options (default) = "" (IFCTEXT)
  General | properties | on 1 object (1 IFCFLOWTERMINAL)
    ApplicationType = "" (IFCTEXT)
    Approvals = "" (IFCTEXT)
    Design country = "Turkey" (IFCTEXT)
    Help = "" (IFCTEXT)
    Manufacturer name = "Vitra" (IFCTEXT)
    Mounting type = "Assembly to floor" (IFCTEXT)
    Product Properties = "Concealed Cistern for Wall-Hung WC Pans Standart Installation Set - Adjusted to 3/6lt 8 cm" (IFCTEXT)
    Product SKU = "768-1850-01" (IFCTEXT)
    Product Type = "Concealed Cistern" (IFCTEXT)
    Product family = "Vitra" (IFCTEXT)
    Product group = "Concealed Cistern for Wall-Hung WC Pans" (IFCTEXT)
    Product manual = "" (IFCTEXT)
    Region Africa = "All" (IFCTEXT)
    Region Antarctica = "All" (IFCTEXT)
    Region Asia = "All" (IFCTEXT)
    Region Europe = "All" (IFCTEXT)
    Region Middle East = "All" (IFCTEXT)
    Region North America = "All" (IFCTEXT)
    Region Oceania = "All" (IFCTEXT)
    Region South America = "All" (IFCTEXT)
    Warranty Period (Year) = "10 Years" (IFCTEXT)
    Weight Net (kg) = "8" (IFCTEXT)
  Materials and Finishes | properties | on 1 object (1 IFCFLOWTERMINAL)
    Coating Material = "Console" (IFCLABEL)
    Primary Material = "Orange" (IFCLABEL)
    Secondary Material = "White" (IFCLABEL)
    Third Material = "Blue" (IFCLABEL)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Center" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)